**Tata Intra V30**

The all-new compact truck boasts of ‘Premium Tough’ design philosophy which combines rising levels of visual richness and sophistication with robustness and reliability. With our continuous endeavour to offer better and profitable product experiences to customers, we bring to you the next level variant in the Intra range – Intra V30, which will further enhance customer experience with its next levels of performance, drivability and convenience.

**USPs**:

* Class-leading power of 52 kW (70HP) with 1.5L DI engine
* Wide walk through cabin with contemporary fresh looks
* Best-in-class 2690 mm (8.8 feet) long load body suitable for various applications
* Superior driving comfort and ergonomics ensuring a smooth longer journey
* Low turnaround time leading to more trips through enhanced acceleration and pickup
* The Eco switch, a feature which helps to switch the vehicle between normal and eco mode based on the duty cycle & Gear shift advisor which guides the driver to select the correct gear, ensure High fuel economy
* Features: Power steering, mobile charger point, lockable glove box, storage on dashboard and door trims, electronic cluster, car-like interiors

**Applications:** Mineral water distribution, fruits & vegetables, industrial goods, food grains, construction materials (cement bags, tiles, marble, glass, sand, etc.), hardware items, LPG distribution, lubricants, plywood, etc.

**Technical Specifications:**

|  |  |
| --- | --- |
| **Parameter** | **Description** |
| Engine | 1.5L DI Engine |
| Max Power | 52 kW (70HP) @ 4000 r/min |
| Max Torque | 140 Nm @ 1800-3000 r/min |
| Clutch Type | Single plate dry friction diaphragm type |
| Gear Box | 5 forward + 1 reverse |
| Front Suspension | Semi-elliptical leaf springs |
| Rear Suspension | Semi-elliptical leaf springs |
| Chassis frame | Frame with hydro formed long members |
| Cab | Boltable full forward body shell |
| Battery | 12V, 55 Ah |
| Service Brakes | Vacuum assisted hydraulic brakes |
| Tyres | 185 R14 LT 8PR |
| Wheel Base | 2450 mm |
| GVW | 2565 kg |
| Payload | 1300 kg |